**RFP** **23-5858**

# Annex 5: FINANCIAL PROPOSAL SUBMISSION FORM

##### **INSTRUCTIONS TO BIDDERS**

In their financial proposal, bidders should detail as much as possible the price requested in response to the technical specifications.

Wherever possible, the unit prices of the individual goods should be indicated, followed by the total amount (including any additional services and any other costs associated with the delivery of the goods).

Good detail in their financial proposal helps bidders to give clarity and transparency to their proposal and makes it easier for SPC to score the proposals received.

The contract to be concluded with the selected bidder must mention all the costs incurred for the execution of the assignment entrusted to him (including insurance, packaging, delivery costs, unloading, etc., where applicable). No additional costs can be claimed from SPC after the contract has been signed.

Bidders must also mention any special conditions relating to the amount of their proposal or the terms of payment.

The financial proposal must be submitted inclusive of taxes in accordance with the applicable legislation. However, the final amount of the awarded contract may be paid to the successful bidder inclusive or exclusive of taxes, depending on the tax exemptions enjoyed by SPC as an intergovernmental organisation in its member countries and territories.

The following form is given as an indication, the bidder may submit its financial proposal to SPC in another format, provided that it complies with the instructions detailed in this RFP/RFQ and in particular:

Bidders may choose to bid either in part of whole depending on the packages or lots that best suit their respective business capability and experience. Bidders must include shipping costs to the identified port of delivery for the respective Packages.

Bidders are to provide CIF Pricing for the respective Package or Lots

##### **BIDDER’S FINANCIAL PROPOSAL – GOODS**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Package 1 - Nanumea Ground Water Gallery Materials** | | | | | | | |
| **Ref. No.** | **Lot 1 - Pipes** | **Unit** | **Qty** | **Rate** | **Total** | |
| P1.01.001 | DN 450 uPVC Pressure Pipe Series 1, PN 9 in 2.5m Segment. *Segment to have two DN 150 Sub Connections located 0.5m from depth open plain end of pipe on opposite sides with other end sealed (end cap or similar approved)* | Each | 1 |  |  | |
| P1.01.002 | DN 450 uPVC Pressure Pipe Series 1, PN 9 in 3m Segment. *Segment to have one end RRJ and other side plain ended* | Each | 1 |  |  | |
| P1.01.003 | DN 150 uPVC Slotted Pipes Series 1, PN 9 (SWJ), 6m Lengths *Slotting pattern as follows: 5 Rows of Slots for Each Pipe Slot Width: 1.0mm Slot Spacing: 10mm Slot Length: 50mm* | Lengths | 40 |  |  | |
| P1.01.004 | DN 100 uPVC Pressure Pipe Series 1, PN 6 (SWJ), 6m Lengths | Lengths | 6 |  |  | |
| P1.01.005 | DN 20 uPVC Pressure Pipe Series 1 PN, 6m Length | Lengths | 2 |  |  | |
| P1.01.006 | DN 50 Polyethylene Pipe PE 100 SDR 21 PN 8 | Lm | 200 |  |  | |
| P1.01.007 | DN 75 Polyethylene Pipe PE 100 SDR 21 PN 8 | Lm | 90 |  |  | |
| P1.01.008 | DN 110 Polyethylene Pipe PE 100 SDR 21 PN 8 | Lm | 150 |  |  | |
| P1.01.009 | DN 100 mPVC Pressure Pipe Series 2, PN 12 (RRJ), 6m Lengths | Lengths | 270 |  |  | |
| **Total Lot 1 - Pipes** | | | | | |  | |
|  | | | | | | | |
| **Ref. No.** | **Lot 2 - Poly Fittings / Components** | **Unit** | **Qty** | **Rate** | **Total** | |
| P1.02.001 | DN 110 - 90 Degree Metric Compression Elbow | Each | 8 |  |  | |
| P1.02.002 | DN 110 - 90 Degree Metric Compression Tee | Each | 5 |  |  | |
| P1.02.003 | DN 110 x 2" BSP Metric Compression Female Adaptor | Each | 10 |  |  | |
| P1.02.004 | DN 110 - Metric Slip / Repair Coupling | Each | 5 |  |  | |
| P1.02.005 | DN 75 x DN 50 Metric Reducer | Each | 1 |  |  | |
| P1.02.006 | DN 75 x 3" BSP Metric Compression Male Adaptor | Each | 6 |  |  | |
| P1.02.007 | DN 75 - 90 Degree Metric Compression Elbow | Each | 8 |  |  | |
| P1.02.008 | DN 75 - 90 Degree Metric Compression Tee | Each | 4 |  |  | |
| P1.02.009 | DN 75 x 3" BSP 90 Degree Metric Compression Elbow | Each | 1 |  |  | |
| P1.02.010 | DN 75 x 2" BSP 90 Degree Metric Compression Elbow | Each | 2 |  |  | |
| P1.02.011 | DN 50 x 1 1/2" BSP Metric Compression Male Adaptor | Each | 1 |  |  | |
| P1.02.012 | DN 50 x 2" BSP Metric Compression Male Adaptor | Each | 12 |  |  | |
| P1.02.013 | DN 50 x 2" BSP Metric Compression Female Adaptor | Each | 4 |  |  | |
| P1.02.014 | DN 50 x 2" BSP 90 Degree Metric Compression Male Elbow | Each | 4 |  |  | |
| P1.02.015 | DN 50 x 2" BSP 90 Degree Metric Compression Female Elbow | Each | 8 |  |  | |
| P1.02.016 | DN 50 - 90 Degree Metric Compression Elbow | Each | 1 |  |  | |
| P1.02.017 | DN 50 - 90 Degree Metric Compression Tee | Each | 2 |  |  | |
| P1.02.018 | DN 50 - 90 Degree Metric Tee with 2" Threaded Female Offtake | Each | 4 |  |  | |
| P1.02.019 | DN 50 - Poly Screen Filter with 2" BSP Threaded Male Ends | No | 3 |  |  | |
| P1.02.020 | DN 50 Air Release Valve (Combination) Triple Action with 2" BSP Male Threaded End | No | 3 |  |  | |
| P1.02.021 | DN 50 Check Valve with 2" BSP Male Threaded Ends | No | 3 |  |  | |
| P1.02.022 | 4" x 3" BSP Threaded Poly Reducing Bush | No | 1 |  |  | |
| P1.02.023 | 3" x 3" BSP Male Threaded Nipple | No | 4 |  |  | |
| P1.02.024 | 2" x 2" BSP Threaded Poly Nipple | No | 4 |  |  | |
| P1.02.025 | 2" x 2" BSP Threaded Poly Socket | No | 3 |  |  | |
| P1.02.026 | 2" x 1" BSP Threaded Poly Reducing Bush | No | 8 |  |  | |
| P1.02.027 | 2" BSP Threaded Tee (Stainless Steel Reinforced) | No | 3 |  |  | |
| P1.02.028 | 3" BSP Poly Tank Connector with Backing Nut and Male Threaded Outlet | No | 6 |  |  | |
| P1.02.029 | 2" BSP Poly Tank Connector with Backing Nut and Male Threaded Outlet | No | 6 |  |  | |
| P1.02.030 | 1" BSP Poly Tank Connector with Backing Nut and Male Threaded Outlet | No | 6 |  |  | |
| P1.02.031 | 10,000L Capacity PE Rota Tank for Portable Water Supply | No | 4 |  |  | |
| **Total Lot 2 - Poly Fittings / Components** | | | | | |  | |
|  | | | | | | | |
| **Ref. No.** | **Lot 3 - uPVC Fittings** | **Unit** | **Qty** | **Rate** | **Total** | |
| P1.03.001 | DN 150 uPVC Socket Coupler (SWJ) | Each | 4 |  |  | |
| P1.03.002 | DN 150 UPVC Plain Ended End Cap (SWJ) | Each | 2 |  |  | |
| P1.03.003 | 100mm Extra High Tank Overflow Kit (Rainwater Harvesting). Kit to be supplied complete with 100mm Rubber Gasket, Extra High Tank Overflow, 100mm Insect Proof Screen & Stainless-Steel Tank Fittings | Each | 6 |  |  | |
| P1.03.004 | 100mm High Flow Insect Proof Flap with Stainless Steel Screen Moulded into a 4" Male and Female PVC Fittings | Each | 6 |  |  | |
| P1.03.005 | 100mm uPVC 90 Degree Elbow (SWJ) | Each | 12 |  |  | |
| P1.03.006 | 100mm uPVC Straight Coupling (SWJ) | Each | 12 |  |  | |
| **Total Lot 3 - uPVC Fittings** | | | | | |  | |
|  | | | | | | | |
| **Ref. No.** | **Lot 4 - Metallic Fittings** | **Unit** | **Qty** | **Rate** | **Total** | |
| P1.04.001 | DN 80 Stainless Steel Lockable Ball Valve with 3" BSP Threaded Female Ends | No | 5 |  |  | |
| P1.04.002 | DN 50 Multi jet Flow Meter with 2" BSP Male Threaded Connectors | No | 1 |  |  | |
| P1.04.003 | DN 50 Float Valve With Brass Piston and Backing Nut (2" BSP Threaded End) | No | 5 |  |  | |
| P1.04.004 | DN 50 Stainless Steel Lockable Ball Valve with 2" BSP Threaded Female Ends | No | 7 |  |  | |
| P1.04.005 | DN 25 Stainless Steel Lockable Ball Valve with 2" BSP Threaded Female Ends | No | 6 |  |  | |
| P1.04.006 | DN 25 Bib Tap with 1" BSP Threaded Outlet | No | 6 |  |  | |
| P1.05.009 | DN 100 Tapping Band with 50mm BSP Bore | Each | 1 |  |  | |
| **Total Lot 4 - Mechanical Fittings** | | | | | |  | |
|  | | | | | | | |
| **Ref. No.** | **Lot 5 - Ductile Iron Fittings** | **Unit** | **Qty** | **Rate** | **Total** | |
| P1.05.001 | DN 100 x DN 80 Ductile Iron Concentric Reducer, PN 16, FL - FL | Each | 1 |  |  | |
| P1.05.002 | DN 100 x 90 Degree Ductile Iron Bend, PN 16, FL - FL | Each | 9 |  |  | |
| P1.05.003 | DN 100 x 45 Degree Ductile Iron Bend, PN 16, FL - FL | Each | 1 |  |  | |
| P1.05.004 | DN 100 Ductile Iron All Equal Flanged Tee, PN 16 | Each | 1 |  |  | |
| P1.05.005 | DN 100 Resilient Seated Gate Valve, PN 16 | Each | 2 |  |  | |
| P1.05.006 | DN 100 Ductile Iron Flange Spigot Connector, PN 16, FL - FL | Each | 10 |  |  | |
| P1.05.007 | DN 100 Fully Restrained, Multi-fit Pipe Coupling, PN 16, Complete with Liner (Sealing Range: 104 - 132mm) | Each | 4 |  |  | |
| P1.05.008 | DN 100 Universal Straight Coupling, PN 16  (Sealing Range: 109 - 133mm) | Each | 22 |  |  | |
| P1.05.009 | DN 100 Stainless Steel Dressing Set & Gasket, PN 16 | Each | 21 |  |  | |
| P1.05.010 | DN 80 x 1000mm Ductile Iron Flanged Spool, PN 16 | Each | 1 |  |  | |
| P1.05.011 | DN 80 Underground Fire Hydrant, Squat Type, PN 16 | Each | 1 |  |  | |
| P1.05.012 | DN 80 Fully Restrained Multi-fit Pipe Flange Adaptor (DN 80 Flange, DN65 Socket), PN 16, Complete with Liner. (Sealing Range 71 - 88mm) | Each | 8 |  |  | |
| P1.05.013 | DN 80 Woltmann Type Water Meter, PN 16 | Each | 1 |  |  | |
| P1.05.014 | DN 80 Stainless Steel Dressing Set & Gasket, PN 16 | Each | 16 |  |  | |
| **Total Lot 5 - Ductile Iron Fittings** | | | | | |  | |
|  | | | | | | | |
| **Ref. No.** | **Lot 6 - Timber** | ***Unit*** | ***Qty*** | **Rate** | **Total** | |
| P1.06.001 | 150 x 50mm Pine H3 Grade Rough Cut Timber x 6m Lengths | Lengths | 10 |  |  | |
| P1.06.002 | 75 x 50mm Pine H3 Grade Rough Cut Timber x 6m Lengths | Lengths | 38 |  |  | |
| P1.06.003 | 50 x 50 Pine H3 Grade Rough Cut Timber x 6m Lengths | Lengths | 20 |  |  | |
| P1.06.004 | Marine Ply (2400 x 1200 x 6.5mm) | Sheet | 12 |  |  | |
| P1.06.005 | Non-Structural Form seal Ply (2440 x 1220 x 18mm) | Sheet | 32 |  |  | |
| **Total Lot 6 - Timber** | | | | | |  | |
|  | | | | | | | |
| **Ref. No.** | **Lot 7 - Mechanical Fixings** | **Unit** | **Qty** | **Rate** | **Total** | |
| P1.07.001 | 50mm x 9m 2.5T Heavy Duty Tie Down Ratchet | No | 8 |  |  | |
| P1.07.002 | M10 x 100mm Anchor Bolt Plus Sleeve Anchor Eye Bolt | No | 20 |  |  | |
| P1.07.003 | M10 x 100mm Anchor Bolt Plus Sleeve Hex Nut Bolt | No | 10 |  |  | |
| P1.07.004 | M16 x 100mm Anchor Bolt Plus Sleeve Anchor Hex Nut Bolt | No | 30 |  |  | |
| P1.07.005 | U Bolt 18 x 1/2: with 6" Plate and Nut | No | 12 |  |  | |
| P1.07.006 | 2 Piece Stainless Steel Vertical Pipe Support for DN 50 Poly Pipe complete with fixings (Distance from Base to Pipe Invert - 300mm) | No | 8 |  |  | |
| **Total Lot 7 - Mechanical Fixings** | | | | | |  | |
|  | | | | | | | |
| **Ref. No.** | **Lot 8 - Building Materials** | **Unit** | **Qty** | **Rate** | **Total** | |
| P1.08.001 | General Purpose Blended Cement (40kg Bags) | No | 198 |  |  | |
| P1.08.002 | Deform Bars Grade 500 High Tensile 12mm x 6m Lengths | Ton | 2.7 |  |  | |
| P1.08.003 | 200 micron Builders Plastic (1820mm x 60m) | Rolls | 8 |  |  | |
| P1.08.004 | Non-Woven Geotextile (A14 Bidem or Approved Equivalent) 2000mm Width | Lm | 210 |  |  | |
| P1.08.005 | River Sand | m3 | 11.5 |  |  | |
| P1.08.006 | 5mm River Aggregate | m3 | 40 |  |  | |
| P1.08.007 | 20mm Aggregates | m3 | 13.4 |  |  | |
| P1.08.008 | Bar Chair Slab-On-Ground 75/90mm | Each | 3750 |  |  | |
| P1.08.009 | 100mm Flat Head Bright | Kg | 4 |  |  | |
| P1.08.010 | 75mm Jolt Head Nails | Kg | 9 |  |  | |
| P1.08.011 | Binding Wire 14 Gauge | Kg | 6 |  |  | |
| P1.08.012 | Galvanised Pipe A Grade 20 x 1.6mm x 5.6 Light Plain End | Each | 1 |  |  | |
| **Total Lot 8 - Building Materials** | | | | | |  | |
|  | | | | | | | |
| **Ref. No.** | **Lot 9 - Solar Pump & Accessories** | **Unit** | **Qty** | **Rate** | **Total** | |
| P1.09.001 | Submersible Solar Pump with Helical Rotar & 50m Pumping Head. The Pump Set is to be supplied complete with Motor Controller, and all associated fittings, including cabling for control unit, pump and PV Panel, accessories, well probe, check valve, pump support, PV Panels & Power Coated Aluminium Fixed Angle Modular Solar Panel Frame as per the manufacture’s specifications and requirements | Item | 1 |  |  | |
| **Total Lot 9 - Solar Pump & Accessories** | | | | | |  | |
|  | | | | | | | |
| **Ref. No.** | **Lot 10 - Consumables / Miscellaneous Items** | **Unit** | **Qty** | **Rate** | **Total** | |
| P1.10.001 | 4" Pressure Gauge (Range 0 - 100) mH2o Scale with Copper Alloy wetted parts & Stainless-Steel Casing. 1" BSP Threaded Male Outlet | Each | 1 |  |  | |
| P1.10.002 | Detectable Blue Underground Marking Tape (Blue Background, "Danger" Buried Water Mains Below") 100mm Wide Tape | Lm | 2200 |  |  | |
| P1.10.003 | Denso Tape | Roll | 10 |  |  | |
| P1.10.004 | Bactericidal Pipe Joint Lubricant | Kg | 10 |  |  | |
| P1.10.005 | DN 100 Spare Rubber Ring for RRJ Socket | Each | 50 |  |  | |
| P1.10.006 | Thread Seal Tape 12mm x 0.08mm x 10m | Each | 260 |  |  | |
| P1.10.007 | Tarpaulin 30 x 40ft Sliver 120 gsm | Each | 4 |  |  | |
| P1.10.008 | PVC Solvent Cement (1L Container) | Litre | 5 |  |  | |
| P1.10.009 | PVC Clear Primer | Litre | 5 |  |  | |
| P1.10.010 | 4" Paint Brush | Each | 4 |  |  | |
| P1.10.011 | Rust Arrest Alkyd Anti-Corrosive Primer | Liter | 2 |  |  | |
| P1.10.012 | 12mm x 250m Nylon Rope | Coil | 1 |  |  | |
| P1.10.013 | 12mm x 20m PE Rope | Coil | 4 |  |  | |
| P1.10.014 | String Line Reel with Rewind Hand Crank (3mm x 41m) | Each | 5 |  |  | |
| P1.10.015 | Paint Roller Tray (285mm) | Each | 6 |  |  | |
| P1.10.016 | Paint Roller Handle (230mm) | Each | 6 |  |  | |
| P1.10.017 | Roller Sleeve 9" x 1/4" | Each | 24 |  |  | |
| P1.10.018 | 50mm High Security Solid Brass Padlock | No | 2 |  |  | |
| P1.10.019 | Rectangular Meter Box, Heavy Duty. Min 425L x 225W x 315H | Each | 2 |  |  | |
| P1.10.020 | 50mm x 9m 2.5T Heavy Duty Tie Down Ratchet | Each | 8 |  |  | |
| **Total Lot 10 - Consumables / Miscellaneous Items** | | | | | |  | |
|  | | | | | | | |
| **Ref. No.** | **Lot 11 - Tools & Equipment** | **Unit** | **Qty** | **Rate** | **Total** | |
| P1.11.001 | Valve T Key | Each | 4 |  |  | |
| P1.11.002 | 28" 6.2Kw Chainsaw | No | 1 |  |  | |
| P1.11.003 | 10" Machete | No | 3 |  |  | |
| P1.11.004 | 14 Piece Metric Ring & Open-End Spanner Set | Set | 4 |  |  | |
| P1.11.005 | 18" Aluminium Pipe Wrench | Each | 4 |  |  | |
| P1.11.006 | 48" Aluminium Pipe Wrench | Each | 4 |  |  | |
| P1.11.007 | 12" Adjustable Wrench (Max Opening 55mm) | Each | 4 |  |  | |
| P1.11.008 | 300mm Hack Saw | Each | 4 |  |  | |
| P1.11.009 | 300mm Hack Saw Blade | Each | 12 |  |  | |
| P1.11.010 | 1800mm x 25mm Hexagonal Crowbar | Each | 15 |  |  | |
| P1.11.011 | Long Handle Plumbers Shovel | Each | 15 |  |  | |
| P1.11.012 | Rotational Pipe Cutter (S-Type) 20 - 75mm | Each | 4 |  |  | |
| P1.11.013 | Rotational Pipe Cutter Spare Blade 20 - 75mm | Each | 4 |  |  | |
| P1.11.014 | Rotational Pipe Cutter (S-Type) 90 - 260mm | Each | 4 |  |  | |
| P1.11.015 | Rotational Pipe Cutter Spare Blade 140/160mm | Each | 4 |  |  | |
| P1.11.016 | Rasp File | Each | 9 |  |  | |
| P1.11.017 | Flat File | Each | 9 |  |  | |
| P1.11.018 | 28 Piece All Purpose Hole Saw Kit | Set | 2 |  |  | |
| P1.11.019 | Fiber Glass Shaft Claw Hammer | Each | 5 |  |  | |
| P1.11.020 | Li-Ion Cordless Brushless 185mm (7") Circular Saw | Each | 2 |  |  | |
| P1.11.021 | 185mm Timber Saw Blade | Each | 6 |  |  | |
| P1.11.022 | 610mm (24") Wrecking Bar | Each | 5 |  |  | |
| P1.11.023 | 10m Measuring Tape | Each | 5 |  |  | |
| P1.11.024 | 300mm Stainless Steel Try Square | Each | 5 |  |  | |
| P1.11.025 | Chalk Line Reel with Red Chalk | Each | 6 |  |  | |
| P1.11.026 | 1200mm Spirit Level | Each | 4 |  |  | |
| P1.11.027 | 10lb Sledgehammer with Graphite Handle | Each | 4 |  |  | |
| P1.11.028 | 14" Abrasive Cut Off Saw | Each | 1 |  |  | |
| P1.11.029 | 14" Cut Off Wheel | Each | 5 |  |  | |
| P1.11.030 | Li-ion Cordless Brushless 125mm (5") Angle Grinder | Each | 2 |  |  | |
| P1.11.031 | 5" Grinding disc | Each | 10 |  |  | |
| P1.11.032 | Li-ion SDS Brushless Rotary Hammer Drill | Each | 2 |  |  | |
| P1.11.033 | Li-Ion Cordless Driver Drill | Each | 2 |  |  | |
| P1.11.034 | 400mm SDS Pointed Chisel | Each | 4 |  |  | |
| P1.11.035 | 18mm x 250mm SDS Concrete Drill Bit | Each | 4 |  |  | |
| P1.11.036 | 14mm x 210mm SDS Concrete Drill Bit | Each | 4 |  |  | |
| P1.11.037 | 12mm x 210mm SDS Concrete Drill Bit | Each | 4 |  |  | |
| P1.11.038 | 20mm x 250mm SDS Flat Chisel | Each | 4 |  |  | |
| P1.11.039 | 500L Capacity Concrete Mixer | Each | 1 |  |  | |
| P1.11.040 | 5.5 HP Petrol Drive Unit | Each | 2 |  |  | |
| P1.11.041 | 9m Submersible Pump Attachment (General Trash Pump) | Each | 2 |  |  | |
| P1.11.042 | 2" x 30m lay Flat Hose with 2" Female Camlock and Hose Clip to match Submersible Pump Outlet | Each | 2 |  |  | |
| P1.11.043 | 30mm x 6m Flexshaft Steel Tip Concrete Vibrator | Each | 2 |  |  | |
| P1.11.044 | Clamped Handle Concrete Screed | Each | 4 |  |  | |
| P1.11.045 | 500mm Concrete Place Push Rake | Each | 4 |  |  | |
| P1.11.046 | 280mm x 120mm Square Trowel | Each | 4 |  |  | |
| P1.11.047 | 355mm x 100mm Pointed Trowel | Each | 4 |  |  | |
| P1.11.048 | 100mm x 270mm Tamping Rammer | Each | 2 |  |  | |
| P1.11.049 | 2750mm - 5000mm Telescoping Aluminium Handle | Each | 4 |  |  | |
| P1.11.050 | Wheelbarrow 100L Capacity | Each | 6 |  |  | |
| P1.11.051 | 5.5kVA Single Phase Generator | Each | 2 |  |  | |
| P1.11.052 | 4T 4m Round Lifting Sling | Each | 2 |  |  | |
| P1.11.053 | 16 kg Demolition Hammer | Each | 1 |  |  | |
| P1.11.054 | 30mm Hex 700mm Bull Point Demolition Drill Bit | Each | 5 |  |  | |
| P1.11.055 | 150kg Aluminium Double Sided Step Ladder (Closed Dimensions: 2760mm x 680mm x 195mm, Open Dimension: 2615mm x 1810mm x 210mm) | Each | 1 |  |  | |
| P1.11.056 | 18V Dual Port Charger for Li-Ion Batteries | Each | 3 |  |  | |
| P1.11.057 | Li-Ion 18V (5.0Ah) Batteries | Each | 14 |  |  | |
| P1.11.058 | 30m Heavy Duty Extension Lead | Each | 4 |  |  | |
| P1.11.059 | 6.5kW 8KVA 4 Stroke Electric Start Generator | Each | 1 |  |  | |
| P1.11.060 | Jerry Can 20L White with Red Lid | Each | 10 |  |  | |
| P1.11.061 | Toolbox | Each | 6 |  |  | |
| **Total Lot 11 - Tools & Equipment** | | | | | |  | |
|  | | | | | | | |
| **Ref. No.** | **Lot 12 - Personal Protective Equipment** | **Unit** | **Qty** | **Rate** | **Total** | |
| P1.12.001 | XXL Hi Viz Vest Compliant with AS/NZS 4602 | Each | 18 |  |  | |
| P1.12.002 | Tinted Safety Glasses | Each | 18 |  |  | |
| P1.12.003 | Caution Black on Yellow Tape (100m x 75mm) | Roll | 4 |  |  | |
| P1.12.004 | Orange Barrier Mesh 1m x 50m (8kg) | Roll | 4 |  |  | |
| P1.12.005 | Vented Hard Hat with Rachet Harness - White (to AS/NZS 1801) | Each | 18 |  |  | |
| P1.12.006 | Shade Halo Plastic Hard Hat Brim - Orange | Each | 18 |  |  | |
| **Total Lot 12 - Personal Protective Equipment** | | | | | |  | |
|  |  |  |  |  |  | |
| **Ref. No.** | **Lot 13 - Prefabricated Items** | **Unit** | **Qty** | **Rate** | **Total** | |
| P1.13.001 | Pump Lifting Rail, (50mm Dia x 3.2mm Thick Galvanised Pipe welded to 10mm thick MS Plate on both ends of pipe with 4 affixed to Wall by 4 x M10 x 100mm Long Anchor Bolts, Overall 1m length) | Item | 1 |  |  | |
| P1.13.002 | Prefabricated Aluminium Chamber Access Hatch with provision for locking, opening 1500mm x 1000mm complete with recessed locking provision and hinge system). All metallic surfaces to be finished with Resene Armourcote 515 HS fast drying epoxy or approved equivalent, Applied in 2 coats at 100-micron thickness per coat | Item | 1 |  |  | |
| **Total Lot 14 - Prefabricated Items** | | | | | |  | |

|  |  |
| --- | --- |
| **Summary of Price Schedule**  **Package 1- Nanumea Groundwater Gallery** | |
| Lot 1 - Pipes |  |
| Lot 2 – Poly Fittings / Components |  |
| Lot 3 – uPVC Fittings |  |
| Lot 4 – Metallic Fittings |  |
| Lot 5 – Ductile Iron Fittings |  |
| Lot 6 – Timber |  |
| Lot 7 – Mechanical Fixings |  |
| Lot 8 – Building Materials |  |
| Lot 9 – Solar Pump & Accessories |  |
| Lot 10 – Consumables / Miscellaneous Items |  |
| Lot 11 – Tools & Equipment |  |
| Lot 12 – Personal Protective Equipment |  |
| Lot 13 – Prefabricated Items |  |
| Other Charges |  |
| **GRAND TOTAL – PACKAGE 1** |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Package 2 - Wotje Ground Water Gallery Materials** | | | | | |
| **Ref. No.** | **Lot 1 - Pipes** | **Unit** | **Qty** | **Rate** | **Total** |
| P2.01.001 | DN 450 uPVC Pressure Pipe Series 1, PN 9 in 2.5m Segment. *Segment to have two DN 150 Sub Connections located 0.5m from depth open plain end of pipe on opposite sides with other end sealed (end cap or similar approved)* | Each | 1 |  |  |
| P2.01.002 | DN 450 uPVC Pressure Pipe Series 1, PN 9 in 2.5m Segment. *Segment to have one end RRJ and other side plain ended* | Each | 1 |  |  |
| P2.01.003 | DN 150 uPVC Slotted Pipes Series 1, PN 9 (SWJ), 6m Lengths. *Slotting pattern to be as follows: 5 Rows of Slots for Each Pipes Slot Width: 1.0mm Slot Spacing: 10mm Slot Length: 50mm* | Lengths | 40 |  |  |
| P2.01.004 | DN 100 uPVC Pressure Pipe Series 1, PN 6 (SWJ), 6m Lengths | Lengths | 6 |  |  |
| P2.01.005 | DN 20 uPVC Pressure Pipe Series 1 PN, 6m Length | Lengths | 2 |  |  |
| P2.01.006 | DN 50 Polyethylene Pipe PE 100 SDR 21 PN 8 | Lm | 200 |  |  |
| P2.01.007 | DN 63 Polyethylene Pipe PE 100 SDR 21 PN 8 | Lm | 10 |  |  |
| P2.01.008 | DN 75 Polyethylene Pipe PE 100 SDR 21 PN 8 | Lm | 50 |  |  |
| P2.01.009 | DN 110 Polyethylene Pipe PE 100 SDR 21 PN 8 | Lm | 150 |  |  |
| P2.01.010 | DN 100 mPVC Pressure Pipe Series 2, PN 12 (RRJ), 6m Lengths | Lengths | 205 |  |  |
| **Total Lot 1 - Pipes** | | | | |  |
|  | | | | | |
| **Ref. No.** | **Lot 2 - Poly Fittings / Components** | **Unit** | **Qty** | **Rate** | **Total** |
| P2.02.001 | DN 110 - 90 Degree Metric Compression Elbow | Each | 8 |  |  |
| P2.02.002 | DN 110 - 90 Degree Metric Compression Tee | Each | 5 |  |  |
| P2.02.003 | DN 110 x 2" BSP Metric Compression Female Adaptor | Each | 10 |  |  |
| P2.02.004 | DN 110 - Metric Slip / Repair Coupling | Each | 5 |  |  |
| P2.02.005 | DN 75 x DN 50 Metric Reducer | Each | 1 |  |  |
| P2.02.006 | DN 75 x 3" BSP Metric Compression Male Adaptor | Each | 6 |  |  |
| P2.02.010 | DN 50 x 1 1/2" BSP Metric Compression Male Adaptor | Each | 1 |  |  |
| P2.02.011 | DN 50 x 2" BSP Metric Compression Male Adaptor | Each | 12 |  |  |
| P2.02.012 | DN 50 x 2" BSP Metric Compression Female Adaptor | Each | 1 |  |  |
| P2.02.013 | DN 50 x 2" BSP 90 Degree Metric Compression Male Elbow | Each | 1 |  |  |
| P2.02.014 | DN 50 x 2" BSP 90 Degree Metric Compression Female Elbow | Each | 5 |  |  |
| P2.02.015 | DN 50 - 90 Degree Metric Compression Elbow | Each | 4 |  |  |
| P2.02.016 | DN 50 - Poly Screen Filter with 2" BSP Threaded Male Ends | No | 3 |  |  |
| P2.02.017 | DN 50 Air Release Valve (Combination) Triple Action with 2" BSP Male Threaded End | No | 3 |  |  |
| P2.02.018 | DN 50 Check Valve with 2" BSP Male Threaded Ends | No | 3 |  |  |
| P2.02.019 | 4" x 3" BSP Threaded Poly Reducing Bush | No | 1 |  |  |
| P2.02.021 | 2" x 2" BSP Threaded Poly Nipple | No | 4 |  |  |
| P2.02.022 | 2" x 2" BSP Threaded Poly Socket | No | 3 |  |  |
| P2.02.023 | 2" x 1" BSP Threaded Poly Reducing Bush | No | 1 |  |  |
| P2.02.024 | 2" BSP Threaded Tee (Stainless Steel Reinforced) | No | 3 |  |  |
| P2.02.025 | 2" BSP Poly Tank Connector with Backing Nut and Male Threaded Outlet | No | 6 |  |  |
| P2.02.026 | 1" BSP Poly Tank Connector with Backing Nut and Male Threaded Outlet | No | 6 |  |  |
| P2.02.027 | 5,000L Capacity PE Rota Tank for Portable Water Supply | No | 4 |  |  |
| **Total Lot 2 - Poly Fittings / Components** | | | | |  |
|  | | | | | |
| **Ref. No.** | **Lot 3 - uPVC Fittings** | **Unit** | **Qty** | **Rate** | **Total** |
| P2.03.001 | DN 150 uPVC Socket Coupler (SWJ) | Each | 4 |  |  |
| P2.03.002 | DN 150 UPVC Plain Ended End Cap | Each | 2 |  |  |
| P2.03.003 | 100mm Extra High Tank Overflow Kit (Rainwater Harvesting). Kit to be supplied complete with 100mm Rubber Gasket, Extra High Tank Overflow, 100mm Insect Proof Screen & Stainless-Steel Tank Fittings | Each | 6 |  |  |
| P2.03.004 | 100mm High Flow Insect Proof Flat with Stainless Steel Screen Moulded into a 4" Male and Female PVC Fittings | Each | 6 |  |  |
| P2.03.005 | 100mm uPVC 90 Degree Elbow | Each | 12 |  |  |
| P2.03.006 | 100mm uPVC Straight Coupling | Each | 12 |  |  |
| **Total Lot 3 - uPVC Fittings** | | | | |  |
|  | | | | | |
| **Ref. No.** | **Lot 4 - Metallic Fittings** | **Unit** | **Qty** | **Rate** | **Total** |
| P2.04.001 | DN 50 Multi jet Flow Meter with 2" BSP Male Threaded Connectors | No | 1 |  |  |
| P2.04.002 | DN 50 Float Valve with Brass Piston and Backing Nut (2" BSP Threaded End) | No | 5 |  |  |
| P2.04.003 | DN 50 Stainless Steel Lockable Ball Valve with 2" BSP Threaded Female Ends | No | 7 |  |  |
| P2.04.004 | DN 25 Stainless Steel Lockable Ball Valve with 2" BSP Threaded Female Ends | No | 6 |  |  |
| **Total Lot 4 - Metalic Fittings** | | | | |  |
|  | | | | | |
| **Ref. No.** | **Lot 5 - Ductile Iron Fittings** | **Unit** | **Qty** | **Rate** | **Total** |
| P2.05.001 | DN 100 x DN 80 Ductile Iron Concentric Reducer, PN 16, FL - FL | Each | 1 |  |  |
| P2.05.002 | DN 100 x 90 Degree Ductile Iron Bend, PN 16, FL - FL | Each | 3 |  |  |
| P2.05.003 | DN 100 x 45 Degree Ductile Iron Bend, PN 16, FL - FL | Each | 4 |  |  |
| P2.05.004 | DN 100 x 11.25 Degree Ductile Iron Bend, PN 16, FL - FL | Each | 1 |  |  |
| P2.05.005 | DN 100 Ductile Iron All Equal Flanged Tee, PN 16 | Each | 3 |  |  |
| P2.05.006 | DN 100 Resilient Seated Gate Valve, PN 16 | Each | 6 |  |  |
| P2.05.007 | DN 100 Ductile Iron Flange Spigot Connector, PN 16, FL - FL | Each | 28 |  |  |
| P2.05.008 | DN 100 Fully Restrained, Multi-fit Pipe Coupling, PN 16, Complete with Liner (Sealing Range: 104 - 132mm) | Each | 4 |  |  |
| P2.05.009 | DN 100 Universal Straight Coupling, PN 16  (Sealing Range: 109 - 133mm) | Each | 38 |  |  |
| P2.05.010 | DN 100 Tapping Saddle with 50mm BSP Bore | Each | 1 |  |  |
| P2.05.011 | DN 100 Stainless Steel Dressing Set & Gasket, PN 16 | Each | 42 |  |  |
| P2.05.012 | DN 80 Fully Restrained Multi-fit Pipe Flange Adaptor (DN 80 Flange, DN65 Socket), PN 16, Complete with Liner. (Sealing Range 71 - 88mm) | Each | 5 |  |  |
| P2.05.013 | DN 80 Stainless Steel Dressing Set & Gasket, PN 16 | Each | 5 |  |  |
| **Total Lot 5 - Ductile Iron Fittings** | | | | |  |
|  | | | | | |
| **Ref. No.** | **Lot 6 - Timber** | ***Unit*** | ***Qty*** | **Rate** | **Total** |
| P2.06.001 | 150 x 50mm Pine H3 Grade Rough Cut Timber x 6m Lengths | Lengths | 10 |  |  |
| P2.06.002 | 75 x 50mm Pine H3 Grade Rough Cut Timber x 6m Lengths | Lengths | 38 |  |  |
| P2.06.003 | 50 x 50 Pine H3 Grade Rough Cut Timber x 6m Lengths | Lengths | 20 |  |  |
| P2.06.004 | Marine Ply (2400 x 1200 x 6.5mm) | Sheet | 12 |  |  |
| P2.06.005 | Non-Structural Form seal Ply (2440 x 1220 x 18mm) | Sheet | 32 |  |  |
| **Total Lot 6 - Timber** | | | | |  |
|  | | | | | |
| **Ref. No.** | **Lot 7 - Mechanical Fixings** | **Unit** | **Qty** | **Rate** | **Total** |
| P1.07.001 | M10 x 100mm Anchor Bolt Plus Sleeve Anchor Eye Bolt | No | 18 |  |  |
| P1.07.002 | U Bolt 18 x 1/2: with 6" Plate and Nut | No | 18 |  |  |
| P1.07.003 | 2 Piece Stainless Steel Vertical Pipe Support for DN 50 Poly Pipe complete with fixings (Distance from Base to Pipe Invert - 300mm) | No | 8 |  |  |
| **Total Lot 7 - Mechanical Fixings** | | | | |  |
|  | | | | | |
| **Ref. No.** | **Lot 8 - Building Materials** | **Unit** | **Qty** | **Rate** | **Total** |
| P2.08.001 | General Purpose Blended Cement (40kg Bags) | No | 198 |  |  |
| P2.08.002 | Deform Bars Grade 500 High Tensile 12mm x 6m Lengths | Ton | 2.7 |  |  |
| P2.08.003 | 200 micron Builders Plastic (1820mm x 60m) | Rolls | 8 |  |  |
| P2.08.004 | Non-Woven Geotextile (A14 Bidem or Approved Equivalent) 2000mm Width | Lm | 210 |  |  |
| P2.08.005 | 5mm River Aggregate | m3 | 40 |  |  |
| P2.08.006 | River Sand | m3 | 12.22 |  |  |
| P2.08.007 | 20mm Aggregates | m3 | 13.45 |  |  |
| P2.08.008 | AP 40 Aggregates | m3 | 1.8 |  |  |
| P2.08.009 | Bar Chair Slab-On-Ground 75/90mm | Each | 3850 |  |  |
| P2.08.010 | 100mm Flat Head Bright | Kg | 2 |  |  |
| P2.08.011 | 75mm Jolt Head Nails | Kg | 14 |  |  |
| P2.08.012 | Binding Wire 14 Gauge | Kg | 5 |  |  |
| P2.08.013 | Galvanised Pipe A Grade 20 x 1.6mm x 5.6 Light Plain End | Each | 1 |  |  |
| **Total Lot 8 - Building Materials** | | | | |  |
|  | | | | | |
| **Ref. No.** | **Lot 9 - Solar Pump & Accessories** | **Unit** | **Qty** | **Rate** | **Total** |
| P2.09.001 | Submersible Solar Pump with Helical Rotar & 50m Pumping Head. The Pump Set is to be supplied complete with Motor Controller, and all associated fittings, including cabling for control unit, pump and PV Panel, accessories, well probe, check valve, pump support, PV Panels & Power Coated Aluminium Fixed Angle Modular Solar Panel Frame as per the manufacture’s specifications and requirements | Item | 1 |  |  |
| **Total Lot 9 - Solar Pump & Accessories** | | | | |  |
|  | | | | | |
| **Ref. No.** | **Lot 10 - Consumables / Miscellaneous Items** | **Unit** | **Qty** | **Rate** | **Total** |
| P2.10.001 | 4" Pressure Gauge (Range 0 - 100) mH2o Scale with Copper Alloy wetted parts & Stainless-Steel Casing. 1" BSP Threaded Male Outlet | Each | 1 |  |  |
| P2.10.002 | Detectable Blue Underground Marking Tape (Blue Background, "Danger" Buried Water Mains Below") 100mm Wide Tape | Lm | 1000 |  |  |
| P2.10.003 | Denso Tape | Roll | 10 |  |  |
| P2.10.004 | Bactericidal Pipe Joint Lubricant | Kg | 10 |  |  |
| P2.10.005 | DN 100 Spare Rubber Ring for RRJ Socket | Each | 50 |  |  |
| P2.10.006 | Thread Seal Tape 12mm x 0.08mm x 10m | Each | 260 |  |  |
| P2.10.007 | Tarpaulin 30 x 40ft Sliver 120 gsm | Each | 4 |  |  |
| P2.10.008 | PVC Solvent Cement (1L Container) | Litre | 5 |  |  |
| P2.10.009 | PVC Clear Primer | Litre | 5 |  |  |
| P2.10.010 | 4" Paint Brush | Liter | 4 |  |  |
| P2.10.011 | Rust Arrest Alkyd Anti-Corrosive Primer | Liter | 2 |  |  |
| P2.10.012 | 12mm x 250m Nylon Rope | Coil | 1 |  |  |
| P2.10.013 | 12mm x 20m PE Rope | Coil | 4 |  |  |
| P2.10.014 | String Line Reel with Rewind Hand Crank (3mm x 41m) | Each | 5 |  |  |
| P2.10.015 | Paint Roller Tray (285mm) | Each | 6 |  |  |
| P2.10.016 | Paint Roller Handle (230mm) | Each | 6 |  |  |
| P2.10.017 | Roller Sleeve 9" x 1/4" | Each | 24 |  |  |
| P2.10.018 | 50mm High Security Solid Brass Padlock | No | 2 |  |  |
| P2.10.019 | Rectangular Meter Box, Heavy Duty. Min 425L x 225W x 315H | Each | 2 |  |  |
| P2.10.020 | 50mm x 9m 2.5T Heavy Duty Tie Down Ratchet | Each | 8 |  |  |
| **Total Lot 10 - Consumables / Miscellaneous Items** | | | | |  |
|  | | | | | |
| **Ref. No.** | **Lot 11 - Tools & Equipment** | **Unit** | **Qty** | **Rate** | **Total** |
| P2.11.001 | Valve T Key | Each | 2 |  |  |
| P2.11.002 | 14 Piece Metric Ring & Open End Spanner Set | Set | 2 |  |  |
| P2.11.003 | 18" Aluminium Pipe Wrench | Each | 2 |  |  |
| P2.11.004 | 48" Aluminium Pipe Wrench | Each | 2 |  |  |
| P2.11.005 | 12" Adjustable Wrench (Max Opening 55mm) | Each | 2 |  |  |
| P2.11.006 | 300mm Hack Saw | Each | 2 |  |  |
| P2.11.007 | 300mm Hack Saw Blade | Each | 10 |  |  |
| P2.11.008 | 1800mm x 25mm Hexagonal Crowbar | Each | 5 |  |  |
| P2.11.009 | Long Handle Plumbers Shovel | Each | 5 |  |  |
| P2.11.010 | Rasp File | Each | 4 |  |  |
| P2.11.011 | Flat File | Each | 4 |  |  |
| P2.11.012 | Toolbox | Each | 2 |  |  |
| **Total Lot 11 - Tools & Equipment** | | | | |  |
|  | | | | | |
| **Ref. No.** | **Lot 12 - Manhole Cover & Frame** | **Unit** | **Qty** | **Rate** | **Total** |
| P2.12.001 | DN 600mm Ductile Iron Lockable Manhole Cover Complete with frame system, D400 loading class. The Manhole covering shall have 2 openings of 63mm Dia meter to account for external pipework | Item | 1 |  |  |
| P2.12.002 | 25mm x 3.2mm x 1m Long Galvanised Pipe | Item | 1 |  |  |
| P2.12.003 | Universal Opening Bar (Compatible with P2.10.001) | Each | 4 |  |  |
| **Total Lot 12 - Manhole Cover & Frame** | | | | |  |

|  |  |
| --- | --- |
| **Summary of Price Schedule**  **Package 2- Wotje Groundwater Gallery** | |
| Lot 1 - Pipes |  |
| Lot 2 – Poly Fittings / Components |  |
| Lot 3 – uPVC Fittings |  |
| Lot 4 – Metallic Fittings |  |
| Lot 5 – Ductile Iron Fittings |  |
| Lot 6 – Timber |  |
| Lot 7 – Mechanical Fixings |  |
| Lot 8 – Building Materials |  |
| Lot 9 – Solar Pump & Accessories |  |
| Lot 10 – Consumables / Miscellaneous Items |  |
| Lot 11 – Tools & Equipment |  |
| Lot 12 – Manhole Cover & Frame |  |
| Other Charges |  |
| **GRAND TOTAL – PACKAGE 2** |  |

No payment will be made for items which have not been priced. Such items are deemed to be covered by the financial offer.

Bidders will be deemed to have satisfied themselves, before submitting their proposal and to its correctness and completeness, taking into account of all that is required for the full and proper performance of the contract and to have included all costs in their rates and prices.

|  |
| --- |
| **For the Bidder:** *[insert name of the company]* |
| Signature:  Name of the representative: *[insert name of the representative]*  Title: *[insert Title of the representative]* |
| Date: *[Click or tap to enter a date]* |